# Plot a large network of GNSS data

# Load the data

The data `df_estimated_velocities_gmwmx` contains estimated northward and eastward velocities and their respective standard deviation for a subset of 1202 GNSS station with more than 10 years of daily data.

Let us first load the `gmwmx2` package.

    library(dplyr)
    library(gmwmx2)
    library(sf)

    data("df_estimated_velocities_gmwmx")

    range(df_estimated_velocities_gmwmx$length_signal)

    ## [1]  3681 11169

    # define function to make color transparent
    make_transparent <- function(colors, alpha = 0.5) {
      # Ensure alpha is between 0 and 1
      if (alpha < 0 || alpha > 1) {
        stop("Alpha value must be between 0 and 1")
      }

      # Convert colors to RGB and add alpha
      transparent_colors <- sapply(colors, function(col) {
        rgb_val <- col2rgb(col) / 255
        rgb(rgb_val[1], rgb_val[2], rgb_val[3], alpha = alpha)
      })

      return(transparent_colors)
    }

    countries_sf <- rnaturalearth::ne_countries()

# Plot estimated North/East velocities for all estimated stations

    # plot all stations
    par(mar = c(2.5, 3.5, 1, 1))

    # sett plot limits
    xlims <- c(-180, 180)
    ylims <- c(-90, 90)

    # plot
    plot(NA,
      xlim = xlims, ylim = ylims, las = 1,
      ylab = "", xlab = "",
      xaxt = "n", yaxt = "n"
    )

    # Define longitude labels (X° E/W)
    lon_labels <- sapply(seq(-180, 180, by = 30), function(x) {
      if (x < 0) {
        paste0(abs(x), "° W")
      } else if (x > 0) {
        paste0(x, "° E")
      } else {
        "0°"
      }
    })

    # Define latitude labels (X° N/S)
    lat_labels <- sapply(seq(-90, 90, by = 20), function(y) {
      if (y < 0) {
        paste0(abs(y), "° S")
      } else if (y > 0) {
        paste0(y, "° N")
      } else {
        "0°"
      }
    })

    # Plot the axes
    axis(side = 1, at = seq(-180, 180, by = 30), labels = lon_labels)
    axis(side = 2, at = seq(-90, 90, by = 20), labels = lat_labels, las = 1)

    plot(countries_sf$geometry, add = TRUE, border = "black", lwd = 2)

    # # add axis
    for (i in seq(-180, 180, by = 30)) {
      abline(v = i, col = "grey80", lty = 5)
    }
    for (i in seq(-90, 90, by = 20)) {
      abline(h = i, col = "grey80", lty = 5)
    }

    my_col <- c("#e96bff")
    my_col_trans <- make_transparent(my_col, alpha = .4)

    # set param for graph
    shift <- 0
    scale_arrow <- 200
    arrow_width <- .1
    arrow_lwd <- 2

    for (i in seq(nrow(df_estimated_velocities_gmwmx))) {
      x0 <- as.numeric(df_estimated_velocities_gmwmx[i, "longitude"])
      y0 <- as.numeric(df_estimated_velocities_gmwmx[i, "latitude"])
      x1 <- as.numeric(df_estimated_velocities_gmwmx[i, "longitude"] + df_estimated_velocities_gmwmx[i, "estimated_trend_E_scaled"] * scale_arrow)
      y1 <- as.numeric(df_estimated_velocities_gmwmx[i, "latitude"] + df_estimated_velocities_gmwmx[i, "estimated_trend_N_scaled"] * scale_arrow)

      shape::Arrows(
        x0 = x0, y0 = y0, x1 = x1, y1 = y1,
        col = my_col_trans,
        arr.type = "triangle",
        arr.length = .10,
        arr.width = arrow_width,
        lwd = arrow_lwd
      )
    }

# Zoom in the United States

    # Zoom in the US
    # set plot limits
    xlims <- c(-130, -60)
    ylims <- c(30, 55)

    # plot
    plot(NA,
      xlim = xlims, ylim = ylims, las = 1,
      ylab = "", xlab = "",
      xaxt = "n", yaxt = "n"
    )

    # Define longitude labels (X° E/W)
    lon_labels <- sapply(seq(-180, 180, by = 10), function(x) {
      if (x < 0) {
        paste0(abs(x), "° W")
      } else if (x > 0) {
        paste0(x, "° E")
      } else {
        "0°"
      }
    })

    # Define latitude labels (X° N/S)
    lat_labels <- sapply(seq(-90, 90, by = 10), function(y) {
      if (y < 0) {
        paste0(abs(y), "° S")
      } else if (y > 0) {
        paste0(y, "° N")
      } else {
        "0°"
      }
    })

    # Plot the axes
    axis(side = 1, at = seq(-180, 180, by = 10), labels = lon_labels)
    axis(side = 2, at = seq(-90, 90, by = 10), labels = lat_labels, las = 1)

    plot(countries_sf$geometry, add = TRUE, border = "black", lwd = 2)

    # # add axis
    for (i in seq(-180, 180, by = 10)) {
      abline(v = i, col = "grey80", lty = 5)
    }
    for (i in seq(-90, 90, by = 10)) {
      abline(h = i, col = "grey80", lty = 5)
    }

    my_col <- c("#e96bff")
    my_col_trans <- make_transparent(my_col, alpha = .4)

    # set param for graph
    shift <- 0
    scale_arrow <- 200
    arrow_width <- .1
    arrow_lwd <- 2

    for (i in seq(nrow(df_estimated_velocities_gmwmx))) {
      x0 <- as.numeric(df_estimated_velocities_gmwmx[i, "longitude"])
      y0 <- as.numeric(df_estimated_velocities_gmwmx[i, "latitude"])
      x1 <- as.numeric(df_estimated_velocities_gmwmx[i, "longitude"] + df_estimated_velocities_gmwmx[i, "estimated_trend_E_scaled"] * scale_arrow)
      y1 <- as.numeric(df_estimated_velocities_gmwmx[i, "latitude"] + df_estimated_velocities_gmwmx[i, "estimated_trend_N_scaled"] * scale_arrow)

      shape::Arrows(
        x0 = x0, y0 = y0, x1 = x1, y1 = y1,
        col = my_col_trans,
        arr.type = "triangle",
        arr.length = .10,
        arr.width = arrow_width,
        lwd = arrow_lwd
      )
    }

    my_col_trans2 <- make_transparent(my_col, alpha = .6)
    points(df_estimated_velocities_gmwmx$longitude, df_estimated_velocities_gmwmx$latitude, pch = 16, col = my_col_trans2)